### Fedwire Contingency Test Script

### Saturday, October 5, 2013

|  |  |  |
| --- | --- | --- |
| Step | Time (ET) | Description |
| 1 | 9:30 a.m. | Establish connectivity to the Host |
| 2 | 10:00 a.m. | Begin sending message traffic.  Institutions are instructed to send traffic that mirrors a normal production day utilizing special type code(s) when applicable. |
| 3 | 4:00 p.m. | The shutdown process begins.  Initiation of traffic should cease at this time. |
| 4 | 4:30 p.m. | The test is complete. |